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	Company
	[COMPANY NAME]
	Assessment Ref.
	[DOC REF]

	Assessment Title
	Asbestos
	Revision
	[REV]

	Assessed By
	[ASSESSOR NAME / ROLE]
	Assessment Date
	[DATE]

	Location / Scope
	[LOCATION / SCOPE]
	Review Date
	Within 12 months or on significant change



Risk Rating Methodology (5 × 5): Risk = Likelihood × Severity
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		Low (1-4)
	Acceptable - maintain existing controls and monitor.

	Medium (5-9)
	Tolerable - reduce so far as is reasonably practicable.

	High (10-15)
	Substantial - additional controls required before proceeding.

	Very High (16-25)
	Intolerable - stop activity; immediate action required.






Asbestos Risk Assessment
Initial Risk = risk before / with baseline controls.  Residual Risk = risk once all listed controls are in place.
	Ref
	Hazard
	Who might be harmed & how
	L
	S
	R
	Control measures
	L
	S
	R
	Action owner / target

	A1
	Presence of asbestos-containing materials (ACMs)
	Staff, visitors, contractors and maintenance workers - asbestos-related disease (mesothelioma, asbestosis, lung cancer) from inhaling fibres; long latency and potentially fatal.
	3
	5
	15
	1. Asbestos management survey carried out where the building was constructed or refurbished before 2000
1. Asbestos register held and available
1. Duty to manage under CAR 2012 reg 4 discharged
1. Known ACMs labelled where appropriate
1. Keep the register current
1. Re-inspect known ACMs at planned intervals
	1
	5
	5
	[OWNER / DATE]

	A2
	Disturbance of ACMs during work
	Maintenance staff and contractors - fibre release when drilling, fixing or carrying out intrusive work.
	3
	5
	15
	1. Asbestos register consulted before any intrusive work
1. Permit-to-work system operated
1. Register extract issued to contractors
1. No drilling or fixing into suspect materials without a check
1. Formalise a “check the register before you drill” briefing for everyone carrying out work
	1
	5
	5
	[OWNER / DATE]

	A3
	Damaged or deteriorating ACMs
	All occupants - fibre release from damaged or disturbed materials.
	2
	5
	10
	1. Condition of known ACMs monitored through the management plan
1. Damage reported and the area isolated
1. Remediation carried out by a licensed contractor
1. Provide a clear route to report suspected damage
1. Act promptly on re-inspection findings
	1
	5
	5
	[OWNER / DATE]

	A4
	Contractors unaware of asbestos presence
	Contractors - uninformed disturbance of ACMs.
	2
	5
	10
	1. Register provided to all contractors before work
1. Contractors sign to confirm they have reviewed it
1. Only competent (licensed where required) contractors used
1. Include asbestos awareness in the contractor induction
	1
	5
	5
	[OWNER / DATE]

	A5
	Lack of staff awareness / training
	Staff - inadvertent disturbance of ACMs through lack of awareness.
	2
	4
	8
	1. Asbestos awareness training for those liable to disturb ACMs
1. Management arrangements communicated to staff
1. Maintain training records and refresh periodically
	1
	4
	4
	[OWNER / DATE]

	A6
	Unknown asbestos status / survey overdue
	All occupants - unmanaged risk where the presence of ACMs has not been established.
	2
	5
	10
	1. Post-2000 buildings with no ACMs documented as such
1. Where status is unknown, materials presumed to contain asbestos until surveyed
1. Commission a management survey where none exists or status is uncertain
	1
	5
	5
	[OWNER / DATE]


This risk assessment must be reviewed within 12 months, following any incident or near miss, on significant change to the premises, staff, equipment or working practices, or where there is reason to believe it is no longer valid.

	Assessed by (sign)
	Date
	Reviewed by (sign)
	Date
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